BIOPTI image simulation tool This spreadsheet provides a tool that enables you to simulate how different levels of water quality would be mapped using a range of commercially available imaging sensors. By running the simulation you can determine if your application is possible and which satellite would be best suited to it. The spreadsheet is driven by specifications of the concentrations of absorbing (e.g. chlorophyll) or scattering (e.g. suspended sediment) features you are trying to map and some basic parameters describing the optical properties of the water body you are working in. For more detailed advice please contact Dr. Arnold Dekker (arnold.dekker@csiro.au, phone: 61-2-62465821) Run BIOPTI The Bio-Optical Model for Inland Waters version 1.0 (Microsoft Excel File 1MB)
| Feedback | Copyright | Privacy | Disclaimer © 2006 The University of Queensland, Brisbane, Australia ABN 63 942 912 684, CRICOS Provider No:00025B Authorised by: Head of School Maintained by: RStk@gpa.uq.edu.au Last Updated: 21 June 2006