Satellite radar Close Window

Data type sensor (platform) | Spatial scale extent (GRE) | Spectral resolution | Radiometric resolution | Temporal resolution frequency (time of day) | Source/cost | Archive
Radarsat | Medium (Province Region) Extent: 100km x 100km GRE: 30m | Low C band (5cm) | Not applicable | AM 3-5 days | Geoimage or ACRES US $3500 for georeferenced 100km x 100km scene | Collected since 1995
ERS-1/2 | Medium (Province Region) Extent: 100km x 100km GRE: 10-30m | Low C band (5cm) | AM 35 days | $2200 for georeferenced single scene | Collected since 1995
JERS1 | Medium (Province Region) Extent: 75km x 100km GRE: 18m | Low L band (24cm) | AM 44 days Ceased operation in 2000 | $1500 for georeferenced single scene | Collected 1992–1998, no CRC archive
ASAR (ENVISAT) | Medium (Province Region) Extent: 100km x 100km GRE: 150m | Low L band (24cm) | AM 3-5 days | Not available |