Marine remote sensing toolkit

- Home
- Environments
- Text sequence
- Graphic sequence
- Resources
- Help
- Contacts

BRG The University of Queensland
Graphic sequence
Category: Coastline
Variable: Mean high or low water mark
The sensor and platform types available for mapping coastline at the mean high water mark are displayed in the table below. Click on the figure to view mapping options for the mean low water mark.
Options for mapping or monitoring coastline
Passive imaging systems Airborne digital photography Satellite multispectral, fine resolution Satellite multispectral, medium resolution Airborne hyperspectral Satellite hyperspectral, medium resolution Satellite hyperspectral, coarse resolution Airborne photography Active imaging systems Airborne radar Satellite radar Airborne laser Underwater acoustics Field based Boat-based Diving Snorkelling
Click for data required, processing, constraints and references (pdf).