Marine remote sensing toolkit

- Home
- Environments
- Text sequence
- Graphic sequence
- Resources
- Help
- Contacts

BRG The University of Queensland
Help

- Go back

# Radiometric resolution

Radiometric resolution defines the sensitivity or precision of the imaging sensor and is a quantitative measure of the level of variation in reflected light able to be detected by the sensor. The higher the radiometric resolution, the more detailed changes in reflected light able to be measured. As radiometric resolution is increased more detailed changes in reflected light are able to be measured.