Atmospheric remote sensing toolkit

- Home
- Environments
- Text sequence
- Graphic sequence
- Resources
- Help
- Contacts

CRSSIS The University of Queensland
Fundamentals

- Main page
- Pre-processing
- Field data collection
  - Groundcover sampling
    - Field data sources
    - Photo transects
  - Vegetation structure
  - Spectral libraries
  - Optical properties
  - Control points
  - Features mapping
- Mapping approaches
- Change and trends
- Delivery

# Photo transects: required equipment

The photo below presents an example of field equipment used. The minimum equipment required are: 1 x GPS in dry-bag, float, digital camera in housing, GIS software, software to link photo and GPS.