Atmospheric remote sensing toolkit

- Home
- Environments
- Text sequence
- Graphic sequence
- Resources
- Help
- Contacts

CRSSIS The University of Queensland
Fundamentals

- Main page
- Pre-processing
- Field data collection
  - Groundcover sampling
    - Field data sources
    - Photo transects
    - DGPS surveys
    - Driving surveys
  - Vegetation structure
  - Spectral libraries
  - Optical properties
  - Control points
  - Features mapping
- Mapping approaches
- Change and trends
- Delivery

# Detailed surveys: example stream bank survey

Differential GPS for surveying stream banks: Very precise measurements of location is required when comparing field measurements to airborne laser scanning data. Differential GPS measurements can provide sub-metre accuracy in the field.

Field photos taken along the Brisbane River to determine the exact location of the stream banks.

## Reference:

Insert reference.