Airborne multi & hyperspectral Close Window

Data type sensor (platform) | Spatial scale extent (GRE) | Spectral resolution | Radiometric resolution | Temporal resolution frequency (time of day) | Source/cost | Archive
Airborne multispectral
Specterra DMSV Daedalus-1268 ADAR | Extremely fine to fine (local) Extent: 100km2 GRE: 0.5-3.0m | Medium Range: 250-2500nm #bands: 3-20 | Medium 8 bit (256 levels) | User controlled (subject to weather and aircraft availability) | Contact companies for quotes (approx $2-6/km2 for georeferenced image): Specterra systems AirTarget services | Contact companies for details
Airborne hyperspectral
CASI Hymap | Extremely fine to fine (local) Extent: 100km2 GRE: 0.5-10m | High Range: 400-2500nm #bands: >20 | High >12 bit (4096 levels) | User controlled (subject to weather and aircraft availability) | Contact companies for quotes (approx >$20/km2 for georeferenced image): DSTO (CASI) Hyvista corporation (HYMAP) | Contact companies for details. CASI and HYMAP data held by A. Held CSIRO Land and Water

More information