Effects of water colour and depth The water column acts to attenuate light by features which absorb and scatter light. This affects the ability of remote sensing systems to 'see' what is in or under the water column. Absorption per unit depth is greatest for red light and least at blue wavelengths, hence the 'blue' appearance of the image at 5m on the left. Scattering is controlled by particles in the water and the water itself. Suspended sediment will scatter red light more than other wavelengths, as shown in the image on the right.
Colour spectrum at 5m depth in clear water | Colour spectrum at 5m depth in turbid water
| Feedback | Copyright | Privacy | Disclaimer © 2006 The University of Queensland, Brisbane, Australia ABN 63 942 912 684, CRICOS Provider No:00025B Authorised by: Head of School Maintained by: RStk@gpa.uq.edu.au Last Updated: 11 September 2006